October 14, 2026

Applicability: Braidwood and Bryon 

Internal Release Information:
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]F2026-025
[bookmark: OLE_LINK3]Added a sub-step tab definition for a fifth level sequential sub-step in the Bryon-Braidwood EOP format

· [bookmark: _Hlk167786851][Check this box if a sql query or a data fix applies to this update].

Generic External Release:
	N/A

Plant Specific Information for Release Letter:
Braidwood and Byron EOP format
· Added a sub-step tab definition for a fifth level sequential sub-step
 
Testing Requirements:
Use Braidwood data
· Print ES-1.1 in the Rev. 4 Draft EOP Master Procedure set
· Verify the sub-steps in the RNO of step 25a has letters for the tab instead of numbers (highlighted in screenshot below)
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Changes/Additions to PROMS Manual and Training Videos:
[Do not use this section – for MRV/DMJ use]
· CSM submitted for PROMS User Manual: ____________.
· CSM submitted for training videos: ____________.
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