July 17, 2026

Applicability:  V.C.Summer 


Internal Release Information:
[bookmark: OLE_LINK1][bookmark: OLE_LINK2]F2026-017
Blank line was sometimes missing after the Note and Caution text.  This was a 64-bit build difference that affected the text width calculations. To fix, added one to the defined text width inside the Caution/Note box format settings.  

· [bookmark: _Hlk167786851][Check this box if a sql query or a data fix applies to this update].


Generic External Release:
	N/A


Plant Specific Information for Release Letter:
V.C. Summer EOP and SAMG formats:
· A minor adjustment to the text width of Cautions and Notes was needed to correct word wrapping within the Caution and Note boxes. As a result, some Caution and Note word wrapping may be different from your previous PROMS version.


Testing Requirements:
Use V.C. Summer data
· Update formats
· Print AOP 117.1 and verify on step 10 that there is blank space between the last line of Note text and bottom of the Note box.
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· Print AOP-900.05 and verify in Attachment 27 on step 3 that there is blank space between the last line of Note text and the first item in the equipment list
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Changes/Additions to PROMS Manual and Training Videos:
[Do not use this section – for MRV/DMJ use]
· CSM submitted for PROMS User Manual: ____________.
· CSM submitted for training videos: ____________.
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