August 4, 2026

Applicability: BNPP

Internal Release Information:

[bookmark: OLE_LINK1][bookmark: OLE_LINK2][bookmark: _Hlk167786851]B2026-070 – When there is a  less-then sign (<) followed by a numeric value in a Word attachment (inside of a table), PROMS thinks the user put in an RO token will generate an RO not found error in the following table row who's text contains <U-Name>.

Example: in the 001,002,003,004 NOP procedure set:
[001,002,003,004]-OP-NOP-RC-001 attachment 8
In the first column of the table look for <U-Name>-431-J-VT-0153
that <U-Name> will generate an RO not found error because of the "<0.120G" in the third column on row above it.
· [Check this box if a sql query or a data fix applies to this update].

Generic External Release:
Updated RO Resolution in Word Sections to handle a specific case where there were tables containing less than signs mixed with ROs.

Plant Specific Information for Release Letter:
Updated RO Resolution in Word Sections to handle a specific case where there were tables containing less than signs mixed with ROs.

Testing Requirements:
· Use Barakah
· Open NOP [001,002,003,004]-OP-NOP-RC-001 attachment 8
· Make a change and close and save it
· Print the Section for a Unit
· All ROs should resolve
· Edit attachment 8 – put an invalid RO in it – like <A-JUNK>
[image: ]
· [bookmark: OLE_LINK4]Save it & Print the Section for a Unit
· Other ROs should resolve – that one should come up as RO Not Found
· [image: ]
[bookmark: OLE_LINK3]
Changes/Additions to PROMS Manual and Training Videos:
[Do not use this section – for MRV/DMJ use]
· CSM submitted for PROMS User Manual: ____________.
· CSM submitted for training videos: ____________.
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